Instructions for building the black bear from Forum Hoard #137

1. For best results, glue a piece of black construction paper to the back of the model before cutting out, or use a marker to do the "back" of the legs and the base.
2. Score along the bottom of the feet on both sides.
3. Cut out carefully, including the little lines on the nose that let the front of the nose fold down. (If this is too fiddly for you just trim those parts off.)
3. Curl the model and hook the tabs into each other to keep it curled. The model will sit flat if the hooks are on top of the base, not under it.
4. Pinch the nose a little bit to narrow it. Fold the front down and tuck the flaps in.
5. Enjoy your model.